****

**DECKON PREMIUM METAL CEILINGS**

**LAY-IN SYSTEM**

**DATASHEET**

Technical Info:

Product : aluminium or galvanised steel

Sizes : 600x600mm, 300x600mm, 600x1200mm std

Thickness : 0.50 - 0.70 mm

Surface : electrostatic powder coated

Perforation : none or ∅1.8-2.5mm hole diameter with 10-50-100mm bordure  
Suspension sys : hot dip galvanised steel, black


Edge detail : 20-30mm up-turns, as specified

Fire Resistance : class A as steel




Color : RAL 9016, standard white

Specification:


Lay-in system, also called as “semi-concealed” is formed by allowing ceiling tiles lean on T15/24 as tees are visible but there is a shadow effect. All tiles are demountable manually without any special tool so that the system enables fast and easy access to the ceiling void.   
  
VISUAL



**TECHNICAL DRAWINGS**



**PERFORATIONS**

****

  ****